**SCANIA**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | | | | | | | |
|  | G 410 B6x2\*4NB CHASSIS FOR MOBILE CRANE TYPE PALDRIVE 253-260. | | | | | | | |
|  | | |  |  | | |
|  | | |  |  | | |
|  | |  | | | | | | | |
|  | | **Guided Offering** | | | | | | | |
|  | |  | | | | | | | |
|  | | **Initial selections** | | | | | | | |
|  | | |  | |  |  | |
|  | | | **Application** | | Mobile crane | 02758BC | |
|  | | |  | |  |  | |
|  | | | **Operation** | | Regional | 02759B | |
|  | | |  | |  |  | |
|  | | | **Industry** | | Building & Construction | 02790AG | |
|  | | |  | |  |  | |
|  | | | **Cab type** | | CG17L | 00889FL | |

G-series day cab with low roof. The cab has three boarding steps that make it easy to climb into and out of the cab. An extra seat on the engine tunnel or rest break equipment can be selected as required.The cab is suitable for construction and distribution vehicles, applications where an extra spacious day cab is required.Customer benefitsGood possibilities for storage behind driver area and passenger area. Easy to climb in and out of the cab, thanks to the low cab height and the wide boarding steps. A safe workplace, because the cab is designed as a large safety cage around driver and passenger.The cab is certified in accordance with ECE-R 29.03.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **General** | | | | |
|  |  | | | | |
|  | **Type** | | | | |
|  | |  |  |  |
|  | | **Chassis adaptation** | Basic | 01163B |
|  | |  |  |  |
|  | | **Wheel configuration** | 6x2\*4 | 00448N |
|  | |  |  |  |
|  | | **Chassis height** | Normal | 00272B |
|  | |  |  |  |
|  | | **Suspension system** | Air front + Air rear | 00828B |
|  | |  |  |  |
|  | | **Steering wheel position** | left hand | 00403B |
|  |  | | | | |
|  | **Certificates and plates** | | | | |
|  | |  |  |  |
|  | | **WVTA, Whole Vehicle Type Approval according to EC** | Incomplete | 04049B |
|  | |  |  |  |
|  | | **CO2 declaration data** | with | 07202A |
|  | |  |  |  |
|  | | **Plate language** | English | 00003B |
|  |  | | | | |
|  | **Dimensions** | | | | |
|  | |  |  |  |
|  | | **Chassis width** | 2550 mm | 00058E |
|  | |  |  |  |
|  | | **Max truck height** | 4 meters 96/53/EG | 03239A |
|  | |  |  |  |
|  | | **Axle distance** | 4750 mm | 01406JD |
|  | |  |  |  |
|  | | **Dimension JA/BEP L020 (Bodywork Exchange Parameters)** | 3350 mm | 01537MX |
|  | |  |  |  |
|  | | **Bogie distance rear axle 1-2** | 1350 mm | 05737E |
|  | |  |  |  |
|  | | **Steering angle 1st, RH turn** | 43 max | 01345AR |
|  | |  |  |  |
|  | | **Steering angle 1st, LH turn** | 47 max | 01346BD |
|  |  | | | | |
|  | **Weights** | | | | |
|  | |  |  |  |
|  | | **Legal weight 1st axle** | 9000 kg | 02751E |
|  | |  |  |  |
|  | | **Legal weight 2nd axle** | 11500 kg | 02752GE |
|  | |  |  |  |
|  | | **Legal weight 3rd axle** | 7500 kg | 02753CE |
|  | |  |  |  |
|  | | **GVW legal** | 26000 kg | 06175IQ |
|  | |  |  |  |
|  | | **GVW technical** | 28000 kg | 06177JK |
|  |  | | | | |
|  | **Engine** | | | | |
|  |  | | | | |
|  | **Engine** | | | | |
|  | |  |  |  |
|  | | **Propulsion** | combustion engine | 04034A |
|  | |  |  |  |
|  | | **Fuel** | Diesel | 00520A |
|  | |  |  |  |
|  | | **Emission level** | Euro 6 | 02471J |
|  | |  |  |  |
|  | | **Engine type** | DC13 163 410 hp Euro 6 /Japan Emission 2016 | 00408TF |

Engine type: Straight 6-cylinder diesel engine  
Displacement: 12.7 dm³  
Max. output at 1800 rpm: 410 hp (302 kW)  
Max torque at 900-1340 rpm: 2150 Nm

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **SCR, Selective Catalytic Reduction** | with | 03488A |
|  | |  |  |  |
|  | | **NOx control** | With | 03636A |
|  | |  |  |  |
|  | | **Torque reduction NOx-control** | With | 03719A |
|  | |  |  |  |
|  | | **Oil level indication** | With | 03829A |
|  | |  |  |  |
|  | | **Noise suppression** | 81/82 dBA R51.03 | 00472AF |
|  |  | | | | |
|  | **Air intake** | | | | |
|  | |  |  |  |
|  | | **Air intake** | front | 02253E |
|  | |  |  |  |
|  | | **Cab air filter type** | normal | 08400A |
|  |  | | | | |
|  | **Cooling system** | | | | |
|  | |  |  |  |
|  | | **Coolant freeze point** | Freezing point -40 degrees Celsius | 03925B |
|  |  | | | | |
|  | **Exhaust system** | | | | |
|  | |  |  |  |
|  | | **Exhaust silencer execution** | Compact | 01967D |
|  | |  |  |  |
|  | | **Exhaust outlet, direction** | backwards | 00392B |
|  | |  |  |  |
|  | | **Silencer length** | 623 mm | 04329B |
|  | |  |  |  |
|  | | **Exhaust silencer longitudinal position (XM)** | 2650 mm | 04810E |
|  |  | | | | |
|  | **Gearbox** | | | | |
|  |  | | | | |
|  | **Gearbox** | | | | |
|  | |  |  |  |
|  | | **Gearbox** | GRS895 | 00017TG |

12-speed gearbox with range change and splitter gear and 2 reverse gears.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **Gear selector position** | Steering wheel | 03574B |
|  |  | | | | |
|  | **Opticruise** | | | | |
|  | |  |  |  |
|  | | **Opticruise** | With | 02519A |

Scania Opticruise is an automatic gear changing system for manual gearboxes.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **Performance modes** | Economy, standard, power | 05112A |
|  | |  |  |  |
|  | | **Cruise control with active prediction** | With | 04844A |
|  | |  |  |  |
|  | | **Kickdown** | With | 04370A |
|  | |  |  |  |
|  | | **Starter interlock gearselector** | With | 05735A |
|  |  | | | | |
|  | **Clutch** | | | | |
|  | |  |  |  |
|  | | **Clutch system** | automatic | 03575B |

Automatic clutch control, together with Opticruise, gives a completely automated shifting system.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **Axles** | | | | |
|  |  | | | | |
|  | **Front axles** | | | | |
|  | |  |  |  |
|  | | **Axle weight front, technical** | 9000 kg | 00073T |
|  |  | | | | |
|  | **Rear axles** | | | | |
|  | |  |  |  |
|  | | **Bogie weight, technical** | 19000 kg (11500 + 7500) | 00552AM |
|  | |  |  |  |
|  | | **Rear axle gear** | R780 | 00021AK |
|  | |  |  |  |
|  | | **Rear axle gear ratio** | 2,92 | 00022AZ |
|  | |  |  |  |
|  | | **Differential lock** | with | 00020A |
|  |  | | | | |
|  | **Tag axle** | | | | |
|  | |  |  |  |
|  | | **Tag axle lift** | with | 00086A |
|  | |  |  |  |
|  | | **Tag axle steering disengageable** | with | 07277A |
|  |  | | | | |
|  | **PTO** | | | | |
|  |  | | | | |
|  | **Clutch independent PTO** | | | | |
|  | |  |  |  |
|  | | **Power Take-Off ED** | Prepared | 04827A |

The engine is supplied prepared for power take-off. The preparation consists of an intermediate gear which is fitted in the flywheel housing.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **PTO** | | | | |
|  | |  |  |  |
|  | | **PTO EG rear type** | EG651P | 06392AK |

The EG651P is mounted on the right-hand side of the gearbox at "5 o'clock". The power take-off rotates anticlockwise, seen from the rear, and is designed for direct-mounted equipment with connection DIN 5462. Ratio: 1:1.28 with low split and 1:1.58 with high split.Max. torque 800 Nm. Max. power output in continuous operation without gearbox oil cooling: 80 kWMax. power output in continuous operation with gearbox oil cooling: 120 kWMax. power output in periodic\* operation: 120 kW.\*50% operating time at maximum permitted output and 50% inoperative during 30-minute intervals.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **Fuel tanks** | | | | |
|  |  | | | | |
|  | **General** | | | | |
|  | |  |  |  |
|  | | **Fuel tank, right hand side** | 400W aluminium | 02627WR |
|  | |  |  |  |
|  | | **Fuel tank location** | Normal | 01368B |
|  | |  |  |  |
|  | | **Fuel filler cap** | lockable | 00518A |
|  | |  |  |  |
|  | | **Fuel label according to EC** | with | 07462A |
|  | |  |  |  |
|  | | **Fuel heater** | with | 00557A |
|  | |  |  |  |
|  | | **Fuel splash protection** | With | 03974A |
|  |  | | | | |
|  | **SCR tanks** | | | | |
|  | |  |  |  |
|  | | **SCR heating system** | With | 04287A |
|  | |  |  |  |
|  | | **SCR reductant tank volume side RHS** | 80 dm3 | 04318E |
|  | |  |  |  |
|  | | **SCR reductant tank filler cap** | Lockable | 04334A |
|  |  | | | | |
|  | **Chassis** | | | | |
|  |  | | | | |
|  | **Frame** | | | | |
|  | |  |  |  |
|  | | **Frame, type** | F950 | 00458B |
|  | |  |  |  |
|  | | **Bodywork holes configuration frame** | entire frame length | 07432A |
|  |  | | | | |
|  | **Steering** | | | | |
|  | |  |  |  |
|  | | **Front axle steering system type** | hydraulic | 07281B |
|  | |  |  |  |
|  | | **Steering force 70/311/EEC** | With | 01367A |
|  | |  |  |  |
|  | | **Manoeuvrability according to 97/27/EC** | Yes | 02127A |
|  | |  |  |  |
|  | | **Steering wheel type** | basic with chrome details | 02153G |
|  | |  |  |  |
|  | | **Adjustable steering wheel** | tilt + slide | 02991C |
|  |  | | | | |
|  | **Suspension front** | | | | |
|  | |  |  |  |
|  | | **Air spring height, front** | Normal | 01334A |
|  |  | | | | |
|  | **Suspension rear** | | | | |
|  | |  |  |  |
|  | | **Air suspension rear type** | 2-spring | 03226A |
|  | |  |  |  |
|  | | **Shock absorber rear axle** | With | 02259A |
|  | |  |  |  |
|  | | **Level adjustment speed** | Fast | 02487F |
|  | |  |  |  |
|  | | **Level adjustment control truck/trailer** | Truck | 04029A |
|  | |  |  |  |
|  | | **Alternative predefined chassis levels** | exhausted bellows + 2 memory | 02488F |
|  | |  |  |  |
|  | | **Load transfer according to EC 97/27** | yes | 02972A |
|  | |  |  |  |
|  | | **Load limit** | at 11500 kg | 00084D |
|  | |  |  |  |
|  | | **Load transfer** | with | 01353AA |
|  | |  |  |  |
|  | | **Load transfer, tag axle position** | always down | 01528A |
|  | |  |  |  |
|  | | **Load transfer limit** | 11500 kg | 06028B |
|  | |  |  |  |
|  | | **Load transfer manoeuvring** | max load transfer request | 06029B |
|  | |  |  |  |
|  | | **Speed limitation for load transfer** | 30 km/h | 01911D |
|  | |  |  |  |
|  | | **Axle load display** | Front and rear | 02478A |
|  |  | | | | |
|  | **Anti-roll bar** | | | | |
|  | |  |  |  |
|  | | **Anti-roll bar, front** | Extra stiffness | 00092D |
|  |  | | | | |
|  | **Electrics** | | | | |
|  | |  |  |  |
|  | | **Battery** | 230 Ah | 00095AM |
|  | |  |  |  |
|  | | **Battery position** | Left hand side | 03979A |
|  | |  |  |  |
|  | | **Alternator charge** | 180 A | 01122X |
|  |  | | | | |
|  | **Wheels & Mudguards** | | | | |
|  |  | | | | |
|  | **Tyres** | | | | |
|  | |  |  |  |
|  | | **Tyre type front axle** | 385/65R22.5 Regional Steer Bridgestone Duravis R-STEER 002 | 08905MT |
|  | |  |  |  |
|  | | **Tyre type rear axle** | 315/80R22.5 Regional Drive Bridgestone Duravis R-DRIVE 002 | 08906LG |
|  | |  |  |  |
|  | | **Tyre type tag axle behind drive axle** | 385/65R22.5 Regional Steer Bridgestone Duravis R-STEER 002 | 08908MT |
|  |  | | | | |
|  | **Rims** | | | | |
|  | |  |  |  |
|  | | **Rim type front axle** | 22.5 x 11.75 steel | 05001FA |
|  | |  |  |  |
|  | | **Rim type rear axle** | 22.5 x 9.00 steel | 05002DA |
|  | |  |  |  |
|  | | **Rim type tag axle behind drive axle** | 22.5 x 11.75 steel | 05004FA |
|  |  | | | | |
|  | **Wheel equipment** | | | | |
|  | |  |  |  |
|  | | **Wheel nut cover** | steel stainless | 00148B |

Wheel nut caps in stainless steel.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **Wheel chock** | 2 pieces | 01233B |
|  |  | | | | |
|  | **Mudguard front** | | | | |
|  | |  |  |  |
|  | | **Front mudguard size** | 675 mm | 05071B |
|  | |  |  |  |
|  | | **Spray-suppression according to EU 109/2011** | With | 05828A |
|  | |  |  |  |
|  | | **Spray suppression** | with | 01421A |
|  | |  |  |  |
|  | | **Mudflap, front** | with | 00053C |
|  |  | | | | |
|  | **Brakes** | | | | |
|  |  | | | | |
|  | **Brake system** | | | | |
|  | |  |  |  |
|  | | **Brake category** | AB | 01493AB |
|  | |  |  |  |
|  | | **Brake adaptation** | Rigid | 00039B |
|  | |  |  |  |
|  | | **Wheel brake** | disc | 01405B |
|  | |  |  |  |
|  | | **Brake control combination** | electronic with disc brake | 02647B |
|  | |  |  |  |
|  | | **Hill hold** | hill hold | 03485C |
|  | |  |  |  |
|  | | **ESP, Electronic Stability Programme** | With, disabling | 02439B |
|  | |  |  |  |
|  | | **ESP setting for ABS trailer** | With | 04386A |
|  | |  |  |  |
|  | | **APS, Air Processing System** | Air management | 02458B |
|  | |  |  |  |
|  | | **Parking brake system** | pneumatic | 06171A |
|  | |  |  |  |
|  | | **Parking brake trailer control** | braked by service line | 05848A |
|  |  | | | | |
|  | **Wheel brakes** | | | | |
|  | |  |  |  |
|  | | **Brake chamber type 1st front** | membrane + spring | 00028B |
|  | |  |  |  |
|  | | **Brake chamber type, 1st rear** | membrane + spring | 00008B |
|  | |  |  |  |
|  | | **Brake chamber type trailing tag axle** | membrane + spring | 01175B |
|  |  | | | | |
|  | **Auxiliary brakes** | | | | |
|  | |  |  |  |
|  | | **Auxiliary brake control** | automatic | 06302B |
|  |  | | | | |
|  | **Trailer brakes** | | | | |
|  | |  |  |  |
|  | | **Trailer brake** | with | 00027A |
|  |  | | | | |
|  | **Body and chassis adaptation** | | | | |
|  |  | | | | |
|  | **Rigid** | | | | |
|  | |  |  |  |
|  | | **Drawbeam** | with | 01529C |
|  | |  |  |  |
|  | | **Drawbeam type** | Central DB7A | 01536T |
|  | |  |  |  |
|  | | **Drawbeam position** | retracted 300 mm | 03717J |
|  |  | | | | |
|  | **Bodywork interface** | | | | |
|  | |  |  |  |
|  | | **Bodywork Communication Interface, BCI** | with | 05837A |
|  | |  |  |  |
|  | | **Bodywork info in Instrument Cluster** | With | 03888A |

By means of lamps, sounds and display messages in the instrument cluster the bodywork has many options for providing the driver with information. There is access to 8 lamps, all with the option to indicate with different colours. There are also a number of pre-defined display messages and a total of five different sounds. All information is adapted to Scania's information levels: alarm system, warning, information and status. In order to be able to activate 2 of the 8 positions using sound and colour, the necessary connectors and cable harnesses are fitted at the factory, 03888.For the option to program and activate all 8 positions, BCI control unit, 05837A, and ICL with full functionality, 03888A, must be selected in combination.9 different variants of symbol lens can be ordered via variant code 07331.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Symbol lens instrument cluster** | flatbed truck with crane | 07331G |
|  |  |  |  |
|  | **Bodywork programmable switch preparation** | with | 07682A |

Programmable switch, as well as complete modules, can always be relocated in the instrument panel using SDP3.If Preparation for programmable switch is specified for bodywork, with, 07682A, there is also the option to add new switches. The option creates an extra function in BICT that makes it possible to program the BCI control unit.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Pushbutton BCI reserved quantity** | 2 pcs | 06793B |
|  |  |  |  |
|  | **Switch positions BWE reserved quantity** | 2 | 07128B |

Two space reservations for electrical bodywork switches in the instrument panel.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Cable harness for bodybuilder** | 7+7+7 | 02411F |

Three 7-pin cable harnesses from the bodywork's central electric unit routed under the cab.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Cable harness for bodybuilder frame** | 8 m | 03023D |

Eight metre long bodybuilder cable for connection of equipment to the rear of the frame.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Cable harness for bodybuilder roof** | With | 03024A |

Wiring is pre-routed from the central electric unit, via the passenger side A-pillar to the roof shelf on the driver's side.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Cable harness additional switches** | With | 03314A |

The dashboard is prepared with wiring for 4 extra switches, 2 on each side of the steering wheel.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Remote control engine start** | Prepared | 03313B |

Additional equipment to enable remote control starting of the engine.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **Trailer connections** | | | | |
|  | |  |  |  |
|  | | **Trailer electric connector** | 1x15 pole ISO 12098 | 00664D |
|  |  | | | | |
|  | **Miscellaneous** | | | | |
|  | |  |  |  |
|  | | **Registration plate holder rear type** | Panel | 04499A |
|  |  | | | | |
|  | **Cab exterior** | | | | |
|  |  | | | | |
|  | **Cab general** | | | | |
|  | |  |  |  |
|  | | **Cab suspension** | air comfort | 02521G |

Air Comfort, with 4-point air suspension, integrated shock absorbers and level adjustment.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **Cab tilting** | mechanical | 01659B |
|  |  | | | | |
|  | **Exterior** | | | | |
|  | |  |  |  |
|  | | **Roof rail** | long | 01401E |
|  | |  |  |  |
|  | | **Sun visor, external** | with | 00060A |
|  | |  |  |  |
|  | | **Horn in front, type** | compressed air 118 dB | 05174A |
|  |  | | | | |
|  | **Front bumper** | | | | |
|  | |  |  |  |
|  | | **Front Underrun Protection, FUP directive** | FUP device | 02398B |
|  | |  |  |  |
|  | | **Bumper protrusion** | 0 mm | 04932A |
|  | |  |  |  |
|  | | **Bumper beam vertical position** | high | 05065A |
|  |  | | | | |
|  | **Windows** | | | | |
|  | |  |  |  |
|  | | **Windscreen** | Tinted | 02313A |
|  | |  |  |  |
|  | | **Door window glass type** | single | 05084A |
|  | |  |  |  |
|  | | **Window, rear wall** | without | 00066B |
|  |  | | | | |
|  | **Mirrors** | | | | |
|  | |  |  |  |
|  | | **Rear view mirror glass driver side** | spherical | 04935B |
|  | |  |  |  |
|  | | **Rear view mirror glass passenger side** | spherical | 04936B |
|  | |  |  |  |
|  | | **Rear view mirror type** | A | 04934A |
|  | |  |  |  |
|  | | **Rear view mirror casing shape** | smooth | 06784A |
|  | |  |  |  |
|  | | **Rear view mirror heating** | with | 04937A |
|  | |  |  |  |
|  | | **Rear view mirror electrical adjustable** | passenger and driver side | 05128B |
|  | |  |  |  |
|  | | **Wide angle mirror** | Driver + passenger side | 02181C |
|  | |  |  |  |
|  | | **Close-proximity mirror** | electrical adjusted + heating | 04938C |
|  | |  |  |  |
|  | | **Front view mirror** | electrical adjusted + heating | 01902E |
|  |  | | | | |
|  | **Lock and alarm** | | | | |
|  | |  |  |  |
|  | | **Locking type cab** | remote central locking | 05123C |
|  | |  |  |  |
|  | | **Frequency remote lock** | 433 MHz | 03889A |
|  | |  |  |  |
|  | | **Number of keys/remotes** | Four | 02343B |
|  |  | | | | |
|  | **Lamps** | | | | |
|  | |  |  |  |
|  | | **Headlamp type** | H7 | 02983E |
|  | |  |  |  |
|  | | **Dipped beam automatic** | with | 05058A |
|  | |  |  |  |
|  | | **Headlamp asymmetry** | Right hand | 00474A |
|  | |  |  |  |
|  | | **Daytime Running Light, DRL function** | With LED DRL + position lamps | 03908B |
|  | |  |  |  |
|  | | **Headlamp levelling** | manual | 02415C |
|  | |  |  |  |
|  | | **Headlamp cleaning** | With | 02416A |
|  | |  |  |  |
|  | | **Spotlamp in roof** | with | 05051A |
|  | |  |  |  |
|  | | **Spotlamp in front grille panel** | with | 05052A |
|  | |  |  |  |
|  | | **Fog lamp front type** | LED 3 diods | 06044C |
|  | |  |  |  |
|  | | **End outline marker lamp** | White | 01313A |
|  | |  |  |  |
|  | | **Beacon** | With | 01330A |

Two rotating warning lamps attached to the roof rails on the sides of the cab roof. The lamps are the halogen type.A switch for operating the rotating warning lamps is located in the cab.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Working lamp rear wall cab top** | with | 05900A |
|  |  |  |  |
|  | **Working lamp side below cab** | prepared | 04742B |

Wiring preparation for work lights on the inside of the frame below the cab, left and right-hand sides. Switch on the door panel is included.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Working lamp rear end** | left hand and right hand side preparation | 04743D |
|  |  |  |  |
|  | **Side marker lamps** | Temporarily mounted | 00313B |

Amber-coloured side marker lamps with light-emitting diodes, temporarily fitted on the frame. The bodybuilder or other workshop must fit them in accordance with national legislation in force.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Side marker lamp direction indication** | with | 07176A |

With direction indicators in the side marker lamps. When the driver signals a turn using the direction indicator lever, the side marker lamps flash as well. When the hazard warning signal is activated, the side marker lamps and all direction indicator lamps flash as well.This is a European legal requirement for vehicles more than 9 metres long. Whole Vehicle Type Approval (WVTA) is not met without this.Advantages for the customerSafety: This indicator provides other road users with an earlier warning of forthcoming turns, thereby enhancing safety.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **Taillamp type** | LED | 03981B |
|  | |  |  |  |
|  | | **Taillamp position** | on bracket | 01532A |
|  | |  |  |  |
|  | | **Reverse alarm** | With disabling | 02412B |
|  |  | | | | |
|  | **Cab interior** | | | | |
|  |  | | | | |
|  | **Seats** | | | | |
|  | |  |  |  |
|  | | **Seat category, driver side** | medium A | 01431B |

Air-sprung seat with the option to adjust position, height, inclination, seat cushion length, backrest and damping.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Seat category, passenger side** | basic | 01432C |

Seat with air suspension and integrated safety belt. The following settings are possible: position, height, seat cushion length and backrest.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Seat upholstery driver side** | knitted + woven | 05028B |
|  |  |  |  |
|  | **Seat upholstery passenger side** | knitted + woven | 05029B |
|  |  |  |  |
|  | **Seat adjustable shock absorber driver side** | with | 05022A |
|  |  |  |  |
|  | **Seat heating driver side** | with | 05024A |
|  |  |  |  |
|  | **Seat armrest driver side** | with | 05026A |
|  |  |  |  |
|  | **Warning signal for unconnected seat belt** | lamp and audio signals | 01511C |

Warns with acoustic signal and warning lamp when the driver's safety belt is not buckled and speed exceeds 25 km/h.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **Storages** | | | | |
|  | |  |  |  |
|  | | **Instrument panel additional module** | accessory panel | 06311B |
|  | |  |  |  |
|  | | **Instrument panel table centre position** | with | 07218A |
|  | |  |  |  |
|  | | **Rear wall storage** | Open | 02042D |
|  | |  |  |  |
|  | | **Storage bar** | small | 05210B |
|  | |  |  |  |
|  | | **External storage compartment** | Driver and passenger side | 02530C |
|  |  | | | | |
|  | **Interior** | | | | |
|  | |  |  |  |
|  | | **Wall panel and headlining material** | vinyl | 02299A |
|  | |  |  |  |
|  | | **Door trim panel type** | black plastic | 09109A |
|  | |  |  |  |
|  | | **Sun visor driver door** | blind | 06172B |
|  | |  |  |  |
|  | | **Boarding grab handle colour** | black | 08081A |
|  | |  |  |  |
|  | | **Curtain door & windscreen** | preparation | 00143B |
|  | |  |  |  |
|  | | **Protective mats floor** | rubber | 02162A |
|  | |  |  |  |
|  | | **Mat centre floor** | rubber | 02168A |
|  |  | | | | |
|  | **Instruments** | | | | |
|  | |  |  |  |
|  | | **Instrument panel finish** | hard | 02172E |
|  | |  |  |  |
|  | | **Instrument cluster** | 4 inch screen km/h | 02301P |

Instrument cluster with 4.1" colour display with trip computer and high resolution.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Window winder control activation** | ignition on or unlocked door | 07411A |
|  |  |  |  |
|  | **Tachograph** | smart Stoneridge | 02303ES |

Smart digital tachograph from Stoneridge that permits remote readout.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **Tachograph data upload** | With | 03956A |
|  | |  |  |  |
|  | | **Speed limitation** | 89 km/h | 06445GJ |
|  | |  |  |  |
|  | | **Speed limitation legal** | 90 km/h | 06446H |
|  | |  |  |  |
|  | | **Scania Lane Departure Warning, LDW** | With | 03601A |
|  | |  |  |  |
|  | | **Advanced Emergency Braking, AEB** | With | 04335A |
|  |  | | | | |
|  | **Climate system** | | | | |
|  | |  |  |  |
|  | | **Climate system heating** | with | 05208A |
|  | |  |  |  |
|  | | **Air conditioning** | with | 00097A |
|  | |  |  |  |
|  | | **Climate system control** | automatic | 02200B |
|  | |  |  |  |
|  | | **Auxiliary heating** | WTA cab + engine heater 6 kW | 00118P |
|  |  | | | | |
|  | **Lighting** | | | | |
|  | |  |  |  |
|  | | **Internal lighting** | ambient | 04843C |

Dome lamps with integrated reading lamp. Boarding lamp. Background lighting by cup holder. Lamps in the roof shelf.Supplementary internal lighting can be added by specifying with variant code family 05974 and 05975.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | | | | |
|  | **Communications** | | | | |
|  | |  |  |  |
|  | | **Infotainment system** | 2 DIN with 7 inch screen (Premium) | 05120B |

Infotainment system with 7-inch colour screen and touch function.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  | **Infotainment buttons on steer wheel** | with | 05203A |
|  |  |  |  |
|  | **Infotainment voice control** | with | 05325A |
|  |  |  |  |
|  | **Loudspeaker** | 4 x 20W with dual coil | 02176C |
|  |  |  |  |
|  | **Digital audio broadcast radio** | with | 06079A |
|  |  |  |  |
|  | **Navigation map data region** | Europe | 07754A |
|  |  |  |  |
|  | **Bluetooth** | With | 03885A |
|  |  |  |  |
|  | **USB IP driver side** | USB | 06498A |
|  |  |  |  |
|  | **USB IP centre position** | USB | 06499A |
|  |  |  |  |
|  | **USB charging port on instrument panel passenger side** | with | 05205A |
|  |  |  |  |
|  | **CB radio** | prepared 12V with speaker | 00391D |
|  |  |  |  |
|  | **Communicator** | C300 complete | 03808C |
|  |  |  |  |
|  | **Camera system FFU** | rear camera chassis infotainment screen | 03832H |

Orlaco rear view camera connected to the infotainment system's monitor.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  |  |
|  | | **12/24V sockets** | Basic | 05750A |
|  |  | | | | |
|  | **Manuals** | | | | |
|  | |  |  |  |
|  | | **Driver´s manual language** | German | 06151C |
|  | |  |  |  |
|  | | **Driver's manual extra language** | English | 06152A |
|  |  | | | | |
|  | **Rescue equipment** | | | | |
|  |  | | | | |
|  | **Rescue equipment** | | | | |
|  | |  |  |  |
|  | | **Hose for tyre inflation** | 20 meter | 00035B |
|  | |  |  |  |
|  | | **Jack** | with | 00466E |
|  | |  |  |  |
|  | | **Rescue equipment except fire extinguisher** | with | 00083F |
|  | |  |  |  |
|  | | **Warning triangle** | 2 pieces | 06534B |
|  | |  |  |  |
|  | | **Bulb and tool kit** | with | 05133A |
|  |  | | | | |
|  | **Colour** | | | | |
|  |  | | | | |
|  | **Cab** | | | | |
|  | |  |  |  |
|  | | **Cab paint type** | solid | 06527A |
|  | |  |  |  |
|  | | **Cab colour white** | Ivory White | 06491A |
|  |  | | | | |
|  | **Chassis** | | | | |
|  | |  |  |  |
|  | | **Chassis colour grey** | Sub Grey | 06778AP |
|  |  | | | | |
|  | **Multi Colour Concept (MCC)** | | | | |
|  | |  |  |  |
|  | | **Front grille upper panel colour** | cab colour | 06010A |
|  | |  |  |  |
|  | | **Front grille upper ribs colour** | cab colour | 06021A |
|  | |  |  |  |
|  | | **Front grille lower panel colour** | cab colour | 06022A |
|  | |  |  |  |
|  | | **Front grille lower ribs colour** | cab colour | 06023A |
|  | |  |  |  |
|  | | **Rear view mirror cover painted** | cab colour | 06024A |
|  | |  |  |  |
|  | | **Sun visor external painted** | cab colour | 06026A |
|  |  | | | | |
|  | **Logistics** | | | | |
|  |  | | | | |
|  | **Market logistics** | | | | |
|  | |  |  |  |
|  | | **Country code** | DK - Denmark | 01256DK |