Detailed technical specification

Palfinger Hooklift installation:

* Installation of a the provided T20 Scan unit (pre painted) with the provided installation KIT from Guima
* Mounting of the hydraulic pump and by pass valve, hydraulic tank incl. device (parts are provided)
* Mounting of the provided aluminum side protection (Guima)

Electrical installations:

* Installation of the provided LED side marker lights (provided with truck)
* Mounting and delivery of 4 psc. LED working lights, 2 psc. placed behind the drivers cabin, 2 psc. at chassis rear, all working lights are switchable from drivers cab, switch is provided from chassis producer
* Electric installation of the remote control into the cab

Hydraulic installations:

* Installation and production of the hose lines between control, Palfinger Hooklift, and Pump
* Installation the provided manual rear underride protection

Accessories:

* Filling of the hydraulic tank with mineral oil HLP 32
* Finish work and sealing of the bodywork
* Installation of the provided netbox from Guima
* Installation of the provided VBG 795 air operated trailer coupling with provided rear cross beam
* Installation of the provided VBG 14 poled electric coupling, duomatic and ABS coupling at rear of the chassis

Adjustments and approvals:

* Parameterization of the truck (adjusting of engine rpm for Palfinger Hooklift operation)
* Testing of the installation
* Without any local approvals of truck and Hooklift
* Without any training of operators